HamConnect-Amiga 0.6.6
======================

Open the HamConnect-Amiga drawer and double-click Install. Keep the complete
drawer together because component payloads remain compressed until selected.

Target
------
AmigaOS 3.0 or later, 68020 or faster, 1 MB Chip RAM, 4 MB Fast RAM, and
16 MB free disk space. The current emulator proof covers the installer,
HamTCP, and idle HamNet on that memory profile. Concurrent HamNet+, HamChat,
and physical-card acceptance still need measurement before public release.

What is included
----------------
- HamTCP networking: GPL AmiTCP 3.0b2 socket engine, HamDHCP, HamNTP,
  HamNetworkGuard, and HamTCPControl.
- HamNet Browser 1.0.10 and native HamChat 0.6.5.
- Network Setup with DHCP or manual IP, gateway, and DNS.
- Wi-Fi Networks with WPA2, WPA, Open, saved profiles, and radio country.
- Floating Network Status widget.
- Network Doctor with a ten-step test ladder, one-click repairs, and a
  credential-redacted support report.
- Same-icon Reinstall, Modify, Repair, Update, Roll Back, and Uninstall.
- Signed Stable and Beta update channels. Updates are checked automatically
  but are never installed without the user.
- AmigaGuide, quick start, hardware profiles, and optional user-driver drawer.
  The user-driver drawer has no Workbench icon; use Show All Files only when
  you need to add a separately obtained driver.

Hardware
--------
Bundled profiles cover PiStorm/Emu68 WiFiPi, Prism2, cnet.device, 3c589.device,
and UAE virtual Ethernet. X-Surf, X-Surf-100, Ariadne, A2065, Plipbox, ZZ9000,
Hydra, ENC624J600, PiStorm SANA-II, and PicoWyfy profiles can use a compatible
driver already installed or supplied by the user in the Drivers drawer.
Recognition is not physical validation; only tested combinations will be
advertised as validated.

After installation
------------------
Everything visible is kept in SYS:Internet/HamNet:
HamNet Browser, optional HamChat, Network Setup, Wi-Fi Networks, Network
Status, Network Doctor, HamUpdate, Install, and Docs. HamNet Browser and
HamChat are peer applications, not nested drawers. HamTCP, receipts, backups,
rollback snapshots, and repair files stay inside the product drawer.

Run Install again for maintenance. Uninstall restores networking displaced by
HamConnect. Reinstall, Modify, Repair, and Update preserve HamNet and HamChat
user data. A failed or interrupted transaction is recovered automatically.

AmiSSL
------
HamConnect, HamTCP, HamNet, HamNet+, and HamChat do not require AmiSSL.
AmiSSL is not bundled or installed. An existing AmiSSL installation is left
untouched and can be tested by Network Doctor after the clock is correct.

Documentation
-------------
Open Docs and double-click Read Me or HamConnect.guide.
